	CMHC Housing Model Type

	Housing Model Details
	Zoning By-law 150-85

	Zoning By-law 26-007

	
	
	Permitted Zones
	Special Advisories

For all Models: Within MTSA – no parking required. Email  planning@cambridge.ca to confirm.

	Permitted Zones
	Special Advisories

For All Models: Within MTSA – no parking required. Email  planning@cambridge.ca to confirm.

	Accessory Dwelling Unit 01


	Gross Building Floor Area: 59 sq.m.
1 Bed
1 Bath
Height 1 Storey, 4 m
Building Width 6.5m
Accessible Alternative Available
	All R Zones
All RM Zones
All RR Zones*
	*RR – within this zone, the model is only permitted if it is within the Urban Area. Email  planning@cambridge.ca to confirm. 

Min Lot Width at the Dwelling – 8.9 m (ISY 1.2)


	R1, R2, R3, RR*

	*RR – within this zone, the model is only permitted if it is within the Urban Area. Email  planning@cambridge.ca to confirm. 

Requires Min Lot Width at the Dwelling – 8.9 m (ISY 1.2)

	Accessory Dwelling Unit 02 


	Gross Building Floor Area: 95 sq.m.
3 Bed
1 Bath
Height 1 Storey, 6m
Building Width 8.5m

	None
	n/a
	R1, R2, R3, RR*
	*RR – within this zone, the model is only permitted if it is within the Urban Area. Email  planning@cambridge.ca to confirm. 

Requires a minimum lot frontage of 21 metres or frontage on a laneway or frontage on a street on a through lot

Requires Min Lot Width at the Dwelling – 14.5m (ISY 3)

If on laneway or through lot, Min Lot Width at the Dwelling – 10.9m (ISY 1.2)

	Fourplex 01

				
	Gross Building Floor Area: 362 sq.m.
1-3 Bed/unit
1-1.5 Bath/unit
Height 3 Storeys, 10 m
Building Width 7.5m
Building Depth 17 m
Accessible Alternative Available – 1 bed/1bath model
	All RM Zones

Considered a mixed terrace dwelling for the purposes of zoning regulations. 

	Requires Min Lot Frontage: 30 m

Requires Min Lot Width at the Dwelling for an Interior Lot:  13.5 m (ISY 3)

Requires Min Lot Width at the Dwelling for a Corner Lot:  16.5 m (ISY 3, ESY 6)

Requires Min Lot Depth: 26 m
(FY 6, RY 3)

Unless on a large lot, likely to require a driveway for parking in the rear yard to, or access to a laneway or located on a through lot to accommodate 4 parking spaces. 




	R1, R2, R3

Considered a multiple dwelling for the purposes of zoning regulations. 
	Requires Min Lot Frontage:
R1 – 15m
R2 – 12m
R3 - 30 m

Requires Min Lot Width at the Dwelling for an Interior Lot: 
R1/R2 -   9.9 m (ISY 1.2)
R3 – 13.5 m (ISY 3)

Requires Min Lot Width at the Dwelling for a Corner Lot:
R1/R2 -   14.7 m (ISY 1.2, ESY 6)
R2 – 11.7 m (ISY 1.2, ESY 3)
R3 – 10.5 m (ISY 3, ESY 0)

Requires Min Lot Depth: 
R1 – 30.5 m (FY 6, RY 7.5)
R2 – 27.5 m (FY 3, RY 7.5)
R3 – 29 m(FY 4.5, RY 7.5)


Unless on a large lot, likely to require a driveway for parking in the rear yard to, or access to a laneway or located on a through lot to accommodate 4 parking spaces. 

	Fourplex 02


	Gross Building Floor Area: 303 sq.m.
1-3 Bed/unit
1 Bath/unit
Height 2 Storeys, 8.65 m
Building Width 9.5m
Building Depth 17 m
Accessible Alternative Available – 1 bed/1bath model
	All RM Zones

Considered a mixed terrace dwelling for the purposes of zoning regulations. 

	Requires Min Lot Frontage: 30 m

Requires Min Lot Width at the Dwelling for an Interior Lot:  15.5 m (ISY 3)

Requires Min Lot Width at the Dwelling for a Corner Lot:  18.5 m (ISY 3, ESY 6)

Requires Min Lot Depth: 26 m
(FY 6, RY 3)

Unless on a large lot, likely to require a driveway for parking in the rear yard, or access to a laneway or located on a through lot to accommodate 4 parking spaces. 
	R1, R2, R3

Considered a multiple dwelling for the purposes of zoning regulations.
	Requires Min Lot Frontage:
R1 – 15m
R2 – 12m
R3 - 30 m

Requires Min Lot Width at the Dwelling for an Interior Lot: 
R1/R2 -   11.9 m (ISY 1.2 )
R3 – 15.5 m (ISY 3)

Requires Min Lot Width at the Dwelling for a Corner Lot:
R1/R2 -   16.7 m (ISY 1.2, ESY 6)
R2 – 13.7 m (ISY 1.2, ESY 3)
R3 – 12.5 m (ISY 3, ESY 0)

Requires Min Lot Depth: 
R1 – 30.5 m (FY 6, RY 7.5)
R2 – 27.5 m (FY 3, RY 7.5)
R3 – 29 m (FY 4.5, RY 7.5)

Unless on a large lot, likely to require a driveway for parking in the rear yard, or access to a laneway or located on a through lot to accommodate 4 parking spaces. 

	Sixplex 


	Gross Building Floor Area: 450 sq.m.
1-2 Bed/unit
1 Bath/unit
Height 3 Storeys, 10.65 m
Building Width 8 m
Building Depth 19 m
Accessible Alternative Available – 1 bed/1bath model
	All RM Zones

Considered a mixed terrace dwelling for the purposes of zoning regulations. 

	Requires Min Lot Frontage: 30 m

Requires Min Lot Width at the Dwelling for an Interior Lot:  14 m (SY 3)

Requires Min Lot Width at the Dwelling for a Corner Lot:  17 m (ISY 3, ESY 6)

Requires Min Lot Depth: 28 m
(FY 6, RY 3)

Unless on a large lot, likely to require a driveway for parking in the rear yard, or access to a laneway or located on a through lot to accommodate 4 parking spaces. 

	R1, R2, R3

Considered a multiple dwelling for the purposes of zoning regulations.
	*R1, R2 – within this zone, the model is only permitted if it is on a lot that was vacant or did not contain a legal single detached dwelling or semi-detached dwelling at the time the Zoning By-law came into effect on February 3, 2026. Email  planning@cambridge.ca to confirm. 

Requires Min Lot Frontage:
R1 – 15m
R2 – 12m
R3 - 30 m

Requires Min Lot Width at the Dwelling for an Interior Lot: 
R1/R2 -   10.4 m (ISY 1.2)
R3 – 14 m (ISY 3)

Requires Min Lot Width at the Dwelling for a Corner Lot:
R1/R2 -   15.2 m (ISY 1.2, ESY 6)
R2 – 12.2 m (ISY 1.2, ESY 3)
R3 – 11 m (ISY 3, ESY 0)

Requires Min Lot Depth: 
R1 – 32.5 m (FY 6, RY 7.5)
R2 – 29.5 m (FY 3, RY 7.5)
R3 – 31 m (FY 4.5, RY 7.5)

Unless on a large lot, likely to require a driveway for parking in the rear yard, or access to a laneway or located on a through lot to accommodate 4 parking spaces. 

	Stacked Townhouse 01


CMHC drawings show 2 unit stacked towns on their own individual lots, not on one lot, however this could be modified to be multiples on one lot.
	Gross Building Floor Area: 201 sq.m.
1-3 Bed/unit
1-2 Bath/unit
Height - 3 Storeys, 10 m
Building Width - 5 m (per 2-unit  building)
Building Depth 14 m

	All RM Zones

Considered a mixed terrace dwelling for the purposes of zoning regulations. 

	Requires Min Lot Frontage: 30 m

With 2 Buildings on Single Lot: 
Requires Min Lot Width at the Dwelling for an Interior Lot:  16 m (ISY 3)

Requires Min Lot Width at the Dwelling for a Corner Lot:  19 m (ISY 3, ESY 6)

Requires Min Lot Depth: 23 m
(FY 6, RY 3)

Unless on a large lot, likely to require a driveway for parking in the rear yard, or access to a laneway or located on a through lot to accommodate 4 parking spaces. 

	R1, R2, R3

Considered a multiple dwelling for the purposes of zoning regulations.
	*R1, R2 – within this zone, the model is only permitted if it is on a lot that was vacant or did not contain a legal single detached dwelling or semi-detached dwelling at the time the Zoning By-law came into effect on February 3, 2026. Email  planning@cambridge.ca to confirm. 

Requires Min Lot Frontage of 30 m

With 2 Buildings on Single Lot:
Requires Min Lot Width at the Dwelling for an Interior Lot: 
R1/R2 -   12.4 m (ISY 1.2)
R3 – 16 m (ISY 3)

Requires Min Lot Width at the Dwelling for a Corner Lot:
R1 – 17.2 m (ISY 1.2, ESY 6)
R2 – 14.2 m (ISY 1.2, ESY 3)
R3 – 13 m (ISY 3, ESY 0)

Requires Min Lot Depth: 
R1 – 27.5 m (FY 6, RY 7.5)
R2 – 24.5 m (FY 3, RY 7.5)
R3 – 26 m (FY 4.5, RY 7.5)

Unless on a large lot, likely to require a driveway for parking in the rear yard, or access to a laneway or located on a through lot to accommodate 4 parking spaces. 

	Stacked Townhouse 02

CMHC drawings show 2 unit stacked towns on their own individual lots, not on one lot, however this could be modified to be multiples on one lot.
	Gross Building Floor Area: 237 sq.m.
1-4 Bed/unit
1-2 Bath/unit
Height 3 Storeys, 10 m
Building Width 6 m (per 2-unit stacked building)
Building Depth 14 m
Accessible Alternative Available – 1 bed/1bath model


	All RM Zones

Considered a mixed terrace dwelling for the purposes of zoning regulations. 

	Requires Min Lot Frontage: 30 m

With 2 Buildings on Single Lot: 
Requires Min Lot Width at the Dwelling for an Interior Lot:  18 m (ISY 3)

Requires Min Lot Width at the Dwelling for a Corner Lot:  21 m (ISY 3, ESY 6)

Requires Min Lot Depth: 23 m
(FY 6, RY 3)

Unless on a large lot, likely to require a driveway for parking in the rear yard, or access to a laneway or located on a through lot to accommodate 4 parking spaces. 

	R1, R2, R3

Considered a multiple dwelling for the purposes of zoning regulations.
	*R1, R2 – within this zone, the model is only permitted if it is on a lot that was vacant or did not contain a legal single detached dwelling or semi-detached dwelling at the time the Zoning By-law came into effect on February 3, 2026. Email  planning@cambridge.ca to confirm. 

Requires Min Lot Frontage of 30 m

With 2 Buildings on Single Lot: 
Requires Min Lot Width at the Dwelling for an Interior Lot: 
R1/R2 -   14.4 m (ISY 1.2)
R3 – 18 m (ISY 3)

Requires Min Lot Width at the Dwelling for a Corner Lot:
R1 -  19.2 m (ISY 1.2, ESY 6)
R2 – 16.2 m (ISY 1.2, ESY 3)
R3 – 15 m (ISY 3, ESY 0)

Requires Min Lot Depth: 
R1 – 27.5 m (FY 6, RY 7.5)
R2 – 24.5 m (FY 3, RY 7.5)
R3 – 26 m (FY 4.5, RY 7.5)

Unless on a large lot, likely to require a driveway for parking in the rear yard, or access to a laneway or located on a through lot to accommodate 4 parking spaces. 






